*Radare2 cheat sheet:*

**r2 -d <filename>🡪 debug mode**

iz 🡪 strings

is 🡪 functions

s 🡪 seek to

/ 🡪 search

aaa 🡪 analyze

axt 🡪 get good address

dr zf=0 🡪 set zf to 0

dr zf=1 🡪 set zf to 1

V 🡪 visual mode

pp 🡪 good view

B 🡪 breakpoint

**r2 -w <filename>🡪 write mode**

iz 🡪 strings

is 🡪 functions

s 🡪 seek to

/ 🡪 search

aaa 🡪 analyze

axt 🡪 get good address

V 🡪 visual mode

pp 🡪 good view

B 🡪 breakpoint

wa 🡪 write over an instruction 🡪 need to be in “ ” if you are doing more than 1 and followed my a ;

“wa nop; nop” (“” must be in there)

nop 🡪 no operation 🡪 1 nop = 2 bytes (numbers)

wao 🡪 change a condition 🡪 wao?

wa <condition> <destination address> 🡪 change the target address

wa je 0x0000149e